
***********************************************************************
***
***
***				REQUIREMENTS
***
***
***********************************************************************

O.S. Windows(C), from XP to 10 all versions.

The suite of programs for the management and configuration of BY11300 requires Microsoft .NET Framework 4.
Only if your computer is not installed (frequently in Windows XP),
download and install the Microsoft .NET Framework 4 from the Microsoft website,
in the language of your operating system.

***********************************************************************
***
***
***				IMPORTANT !!!
***
***
***********************************************************************

The setup file does not allow you to choose the location of the files, which are
installed on the disk where Windows resides (eg. C: \) in the subfolder <Bytronic>
which includes all programs and suites that Bytronic will release.
You are strongly advised not to manually move the files or groups of files because
confusions and errors may occur and especially you can have write permissions problems
in subdirectories of each application.
To keep all grouped (programs with only their data) instead of 'spread' data in other directories
(eg. documents) allows a much more careful and precise control of the applications.

If you have an earlier version of software, you MUST uninstall it before upgrading.
This ensures that all components of the suite are correctly installed.

Note: Uninstalling the application does not affect any previously saved data,
      which will find themselves in the same position after installing the new version.
      Contraindications for use of old data with new versions of the application (incompatibility),
      will be reported as required.

-------------------
USE WITH WINDOWS 10
-------------------
The USB-RS232 cable provided by Bytronic use the Prolific PL2303 chip.
It may happen that the serial line is slow, even though the cable driver is updated.
This happens if the system has been migrated to Windows 7, 8 or 10 with the 8.x drivers already installed,
although apparently of the latest version.
In this case it is recommended to go to the website of the manufacturer of the chip
(currently at: http://www.prolific.com.tw/US/ShowProduct.aspx?p_id=225&pcid=41) then download
the zip file with the drivers of the latest version
(currently: http://www.prolific.com.tw/UserFiles/files/PL2303_Prolific_DriverInstaller_v1_12_0.zip)
and run the setup, forcing its complete reinstallation.


-----------------------------------------------------

Update status of .zip-pack Setup_BY11300_Suite_x-x-x-x :

	1-0-0-0		 	14.01.2016	- Release.
						============================================================================
						  Level applications update: (Suite BY11350 1.0.0.0)
						  - BOOT 18F ..........................	1.0.0.9
						  	- Update status of Firmware package: BY11350_1.1.0 - 12.01.2016
						  - Configurator_Editor................	1.0.0.1
						  - Modbus Communicator................	1.0.0.0
						  - GSM Commander......................	1.0.0.0
						  - Hercules Setup Utility ............	3.2.8	
						============================================================================

	1-0-0-1		 	26.02.2016	
						============================================================================
						  Level applications update: (Suite BY11350 1.0.0.1 *CHANGED*)
						  - BOOT 18F ..........................	1.0.0.10 *NEW*
						  	- Update status of Firmware package: BY11350_1.1.1 - 26.02.2016 *NEW*
						  - Configurator_Editor................	1.0.0.1 *UNCHANGED*
						  - Modbus Communicator................	1.0.0.0 *UNCHANGED*
						  - GSM Commander......................	1.0.0.0 *UNCHANGED*
						  - Hercules Setup Utility ............	3.2.8	*UNCHANGED*
						============================================================================
	2-0-0-0		 	14.02.2017	
						============================================================================
						  Level applications update: (Suite BY11350 2.0.0.0 *CHANGED*)
						  - BOOT 18F ..........................	1.0.0.10 *UNCHANGED*
						  	- Update status of Firmware package: BY11350_1.2.0 - 07.02.2017 *NEW*
						  - Configurator_Editor................	3.0.0.0 *NEW* (bi-lingual)
						  - Modbus Communicator................	1.0.0.3 *NEW*
						  - GSM Commander......................	1.0.0.0 *UNCHANGED*
						  - Hercules Setup Utility ............	3.2.8	*UNCHANGED*
						============================================================================
